ICA2 For thought

Team COM.

CSE 5323 Chen, Yu; Mei, Shenxiao.

CSE 7323 Ouyang, Zhenxuan.

1. Yes. It would work properly since we calculate 20 maximum data points based on the size of buffer\_size. As long as buffer\_size is larger than 20, it should automatically divide the buffer into 20 chunks and calculate maximum value out of every chunk.
2. Yes, because of efficiency. When we use the back button on navigation bar to go back the table view, we will deallocate the memory, and it will allocate memory again if we tap the cell. The pause function only invalidates the timer and closes the microphone, and it doesn’t deallocate the memory of the audio manager. Therefore, we can have better efficiency if we use pause function.